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	DEVELOPMENT PROPOSED:
	Installation of 3 x 32,000 litre stainless steel tanks within a bunded area.

	AT:
	Link 59 Business Park Block M Pimlico Link Road Clitheroe Lancs 



	Ribble Valley Borough Council hereby give notice that permission has been granted for the carrying out of the above development in accordance with the application plans and documents submitted subject to the following condition(s):



	1. 
	The development must be begun not later than the expiration of three years beginning with the date of this permission.

Reason:  Required to be imposed pursuant to Section 91 of the Town and Country Planning Act 1990.



	2. 
	Any facilities for the storage of oils, fuels or chemicals shall be sited on impervious bases and surrounded by impervious bund walls, details of which shall be submitted to the Local Planning Authority for approval.  The volume of the bunded compound should be at least equivalent to the capacity of the tank plus 10%.  If there is multiple tankage, the compound should be at least equivalent to the capacity of the largest tank, or the combined capacity of interconnected tanks, plus 10%.  All filling points, vents, gauges and sight glasses must be located within the bund.  The drainage system of the bund shall be sealed, with no discharge to any watercourse, land or underground strata.  Associated pipework should be located above ground and protected from accidental damage.  All filling points and tank overflow pipe outlets should be detailed to discharge downwards into the bund.

Reason:  To prevent pollution of the water environment in accordance with Policy G1 of the Ribble Valley Districtwide Local Plan.

P.T.O.




Relevant planning policy

	Policy G1 - Development Control


	Summary of reasons for approval

The proposal has no significant detrimental impact on nearby residential amenity, nor would it have an adverse visual impact or be to the detriment of highway safety.



	


Note(s)

	1. 
	For rights of appeal in respect of any condition(s)/or reason(s) attached to the permission see the attached notes.



	2. 
	The applicant is advised that should there be any deviation from the approved plan the Local Planning Authority must be informed.  It is therefore vital that any future Building Regulation application must comply with the approved planning application.



	3. 
	Any above ground oil storage tank(s) or chemical storage tank(s) should be sited on an impervious base surrounded by a 'liquid tight' bund wall.  No drainage outlet should be provided.  The bunded area should be capable of containing 110% of the volume of the largest tank and all fill pipes, draw pipes and sight gauges should be enclosed within the curtilage.  The vent pipe should be directed downwards into the bund.

Underground or overground pipelines should be adequately protected against leakage particularly by corrosion.




STEWART BAILEY
DIRECTOR OF DEVELOPMENT SERVICES
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