Ribble Valley Borough Council                                                                  

DELEGATED ITEM FILE REPORT - APPROVAL

	Ref: AD/JS

	Application No: 
	3/2006/0826/P LISTED BUILDING CONSENT

	Development Proposed:
	Repair work comprising replacement of defective brickwork within the “Ecclesiastical” arches (mainly south elevation) located either side of The Sands road at Whalley Viaduct, Whalley. 

	CONSULTATIONS: Parish/Town Council

	Parish Council - No objections to this proposal. 



	CONSULTATIONS: Highway/Water Authority/Other Bodies

	Ancient Monuments Society – The proposed methodology for the repairs seem sensible and no concern is raised. 



	CONSULTATIONS: Nearby Residents

	No representations received



	RELEVANT POLICIES:

	Planning (Listed Buildings and Conservation Areas) Act 1990



	COMMENTS/ENVIRONMENTAL/AONB/HUMAN RIGHTS ISSUES/RECOMMENDATION:

	Whalley Viaduct (opened 1850) is Grade II listed.  The list description refers to 48 round arches on battered piers.Where Riddings Lane passes through there are concentric brick arches and moulded stone imposts – to each side there are arches filled with brickwork with blind lancet recesses. 

The Design and Access Statement states that the extent of repairs will not be clear until the works commence on site.  All defective bricks removed will be replaced with new brick – locally manufactured – to match the existing profiles and colours.  A lime mortar will be used to set the new bricks into place (1:2,  the lime to be fully hydrated NHL5, and sand to be local).  Some “Standard Drawings” refer to the incorporation of cement and it is presumed such reference is superseded by the above mortar specification.

In my opinion, the diagnosis of defects has been thorough.  Proposed repairs appear necessary and considered.



	SUMMARY OF REASONS FOR APPROVAL:

	The proposed works would have an acceptable impact upon the character and setting of the listed building.



	RECOMMENDATION: That conditional LISTED BUILDING CONSENT be granted.


DATE INSPECTED: 














