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	DEVELOPMENT PROPOSED:
	Proposed single storey rear kitchen and utility room extension. Installation of an undergound oil storage tank in the yard and associated works.

	AT:
	3 Brookside Holden Bolton-by-Bowland Lancashire BB7 4PE

	Ribble Valley Borough Council hereby give notice that permission has been granted for the carrying out of the above development in accordance with the application plans and documents submitted subject to the following condition(s):



	1. 
	The development must be begun not later than the expiration of three years beginning with the date of this permission.

Reason:  Required to be imposed pursuant to Section 91 of the Town and Country Planning Act 1990.



	2. 
	The building shall be faced in natural stone and roofed in natural blue slate unless alternative materials have first been agreed in writing with the Local Planning Authority.

REASON:  In accordance with Policies G1 and ENV1 of the Ribble Valley Districtwide Local Plan and the adopted Supplementary Planning Guidance - "Extensions and Alterations to Dwellings" ensuring a satisfactory standard of external appearance given the location of the property in the Forest of Bowland Area of Outstanding Natural Beauty.



	3. 
	Precise specifications and samples of walling and roofing materials and details of any window and door surrounds including materials to be used shall have been submitted to and approved in writing by the Local Planning Authority before their use in the proposed works.

REASON:  In order that the Local Planning Authority may ensure that the materials to be used are appropriate to the locality in accordance with Policy G1 of the Ribble Valley Districtwide Local Plan and the adopted Supplementary Planning Guidance - "Extensions and Alterations to Dwellings".



	4. 
	No development approved by this permission shall be commenced until details of the new underground oil storage tank have been approved by the Local Planning Authority.  The work should be constructed and completed in accordance with the approved plans.

REASON:  To prevent discharge of contaminated drainage or accidental spillages to underground strata or surface waters in accordance with Policy G1 of the Ribble Valley Districtwide Local Plan.

P.T.O.


Relevant planning policy

	Policy G1 - Development Control.

Policy G4 - Settlement Strategy.

Policy ENV1 - Area of Outstanding Natural Beauty.

Policy H10 - Residential Extensions.

Policy SPG - "Extensions and Alterations to Dwellings"


	Summary of reasons for approval

The proposal represents an appropriate form of development and given its design, size and location would not result in visual detriment to the surrounding countryside. 



	


Note(s)

	1. 
	For rights of appeal in respect of any condition(s)/or reason(s) attached to the permission see the attached notes.



	2. 
	The applicant is advised that should there be any deviation from the approved plan the Local Planning Authority must be informed.  It is therefore vital that any future Building Regulation application must comply with the approved planning application.



	3. 
	Underground storage tanks and associated pipe work containing substances included in List 1 of the EC Groundwater Directive (80/68/EEC) should be of double skinned construction and be provided with intermediate leak detection equipment.



	4. 
	Any facilities for the storage of oils should be sited on an impervious base and surrounded by impervious bund walls.  The volume of the bunded compound should be at least equivalent to the capacity of the tank plus 10%.  All filling points, vents, gauges and sight glasses must be located within the bund.  The drainage system of the bund shall be sealed with no discharge to any watercourse, land or underground strata.  Associated pipework should be located above ground and protected from accidental damage.  All filling points and tank overflow pipe outlets should be detailed to discharge downwards into the bund.




STEWART BAILEY
DIRECTOR OF DEVELOPMENT SERVICES
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